|  |  |  |
| --- | --- | --- |
| 1 | 4  3  5  3  2  1  6 | Mount in the sequence below:   1. Stem 2. Disc nipple 3. Stem ring 4. Spring washer 5. Disc 6. Grub screw |
| 2 |  | "Attention" curve pointing upwards.  Use your thumb to push up the disc nipple so that the spring washer is centered.  Screw the disc onto the disc nipple. |
| 3 |  | Use the wrench to lock the disc against the disc nipple. |
| 4 |  | Screw the grub screw tightly to secure the disc. |